Level Sensor Specifications
Max Switching Voltage

200 VDC

Max Switching Current

0.5 A

Min Breakdow Voltage

250 VDC

Operating Life

10^5 operations

wire length

±200mm

Density of the float

0.6

Exterior

Material: Nylon 6.6

Color: Black

Dimensions

90 mm (length)x 22mm (diameter)

Buoyancy dimensions: 90 mm (length)*22mm (diameter)

Mouting

Thickness: 1mm to 5mm

Hole: 22mm diameter

Compatibility

GroLab TankBot

GroLab UserBot

Warranty

1-year limited hardware warranty