# How to Install GroLab™ PowerBoard?

GroLab PowerBoard comes with a analogue timer that is used to control the contactor inside the PowerBoard.

To install the PowerBoard, you need to take the cover of the board out...

In the bottom connectors present inside the PowerBoard, you need to connect your Live wires, Neutral and Earth as presented in the picture.

The maximum input power is 75A, so make sure you use the proper cables to power your GroLab PowerBoard.

The recommended cable for Live/Neutral connection must be lower or equal to AWG10.