Smoke Detector Sensor Specifications
Operating Voltage

12VDC

Operation mode

N.O. (Normaly Open)

Alarm current

35mA at 12VDC

Connections

4 wire

Audiovisual Indicators

Red LED

buzzer

Alarm Output

Relay: N.O. (Normaly Open)

Buzzer: (0.5dB/m (±0.1dB/m)

Exterior

Material: Plastic

Material: Plastic

Color: White

Dimensions

53mm (length) x 103mm (diameter)

Compatibility

GroLab TankBot

GroLab UserBot

Warranty

1-year limited hardware warranty