Peristaltic Pump Specifications
Operating Voltage

12VDC

Consunption

15W

Flow rate

58ml/min (range: 5.2ml/min-90ml/min)

RPM

0.1-1000rpm*

Tube length

175mm lenght (49.5mm exposed)

Tubing Life

≥200h*

Exterior

Material: Plastic pump head + metal

Colors: yellow (plastic)

Dimensions

75x54x40mm

Temperature range

0 to 40°C

Humidity

<80%

Compatibility

GroLab TankBot

Warranty

1-year limited hardware warranty