Peristaltic Pre Assembled Cable Specifications
Max. Voltage

300V

Wire Gauge

22 AWG

Conductor

Quantity: 4

Material: Copper, Bare

Insulation: PVC

Strand: 7/30

Jacket (Insulation)

Material: Copper, Bare

Diameter: 3.18mm

Thickness: 0.381mm

Operating Temperature

-20°C ~ 75°C

Cable Length

2m

Connectors

1 Female Connector 4 pins

1 Male Connector 4 pins

Compatibility

TankBot/SoilBot/PowerBot