### THE HEART & BRAIN OF THE OPERATION

A state of the art growing unit that interacts with other GroLab™ modules simulating the operation of a brain. It is capable to execute hundreds of instructions and to store a large amount of data allowing a detailed analysis about the life cycle of the user’s plants. GroNode will do all the hard work for you and will notify you if a risk situation arises. The only limit to GroNode is your imagination.

### Autonomous

GroNode is a powerful computer that can do hundreds of tasks by itself. You don't need any PC or other third-party device connected to GroNode for it to continue working.

### Monitor & Analysis

Using GroLab™ Software user can monitor, and analyses the climate variables and the devices current state in real time. Charts, grow(s) overview and manual control are just some perks you can use.

### Notifications

When you provide Internet connection to GroNode it can send real time alerts and updates to your e-mail, keeping you updated about the state of your grow(s) anywhere, anytime.

### Remote Control

When connecting the GroNode to a router with an Internet connection, it allows you to activate the GroLab™ system's remote control. This feature grants user access from anywhere at any time through an easy-to-use software. Allowing to fully control all the modules.

### Programmable Procedures

There are two main types of programmable procedures, alarms and schedules. GroNode has the ability to store and execute up to 100 of each type allowing a precise and extensive automation of any grow(s).

### Modular

GroNode is the core of the GroLab™ modular architecture, it is capable of controlling up to 4 modules of each type (PowerBot, TankBot and SoilBot). This makes it easily adaptable to any grow regardless of its size, type, growing medium or growing system.

### Secure

All GroLab™ communications are protected by several security layers, securing your valuable data. By using Open Grow™ private server, your E-mail notifications are also secured, not letting anyone pinpoint your grow(s).

### Data-Logging

GroNode has its own memory that is capable of storing hundreds of thousands of data. With data-logging and data-visualization features, it is possible to do a detailed analysis about the life cycle of the user’s plants.

### Cloud Upload

Connecting GroNode to the Internet allows the user to configure a cloud server to periodically upload the data-log from all sensors/devices.

GroNode Specifications
Dimensions

91mm x 91mm x 28.7mm

Exterior

Casing: Stainless Steel

Colors: Silver

Physical buttons: Reset, NET Reset, FW Update

Power Supply

USB - 5VDC 1000mA

Connections

USB 2.1 type B

Ethernet LAN RJ45

RP-SMA female

Antenna Included

Yes

USB Cable Included

Yes (Type B-A)

USB Cable Length

2 meters

USB Power Adapter Included

Yes (Type A 230AC-5VDC)

Ethernet LAN Cable Included

Yes

Ethernet LAN Cable Length

1.52 meters

Inter-Module Communication

Radio Frequency - 2.4GHz

Battery

CR2032 Lithium 3V 250mAh

Storage Memory

2MB

Audiovisual Indicators

Buzzer single tone

LED RGB

Warranty

2-years limited hardware warranty

GroNode Instruction Manual