Solenoid Valve Specifications
Operating Voltage

12VDC

Operation mode

NC (Normaly Closed)

Response Time

ON = 0.15s

OFF = 0.3s

Estimated Valve life

500 000 cycles

Filter

Stainless Steel inlet

Working Pressure

0.02-0.8MPa

IN/OUT Ports

1/2" screw thread**

Valve Type

Diaphragm (Operated by Servo)

Exterior

Material: Plastic + Metal

Colors: White

Ambient Temperature

+1°C to +45°C

Water Temperature

0°C to +100°C

Humidity

≤95%

Altitude

≤2500 meters

Compatibility

GroLab TankBot

Warranty

1-year limited hardware warranty