### THE VERSATILE SUBSTRATE ANALYZER

SoilBot is a rigorous and versatile substrate analyzer, it is another module that makes part of the GroLab™ family. It is capable to completely monitor the substrate of your plants regardless of whether it is soil, rock wool, coconut or a recurrent dipping of roots in water. Supports up to 4 moisture sensors giving you the possibility to monitor 4 different groups of plants at same time. When combined with PowerBot or TankBot allows you to automate their irrigation processes, keeping the perfect moisture for your plants avoiding water wasting and floods. SoilBot has also support for 2 temperature sensors allowing you a complete substrate analysis and 2 flood detectors that makes the system able to react/notify in case of flood detection. Take the control of your plants substrate with this versatile module!

### Moisture

SoilBot has the ability to monitor any substrate's moisture regardless of whether it is soil, rock wool, coconut or a recurrent dipping of roots in water. That's right SoilBot can also be used in a hydroponic set up! It supports up to 4 moisture sensors giving you the possibility to monitor 4 different groups of plants at same time. When combined with PowerBot or TankBot allows you to automate their irrigation processes, keeping the perfect moisture for your plants avoiding water wasting and floods.

### Temperature

With this versatile module even the substrate temperature can be fully monitored. SoilBot supports 2 temperature sensors that greatly extends its substrate analysis capabilities. By combining SoilBot with PowerBot or Tankbot, it is possible to create procedures to keep substrate temperature at the perfect value for your plants to continue to grow healthier.

### Flood Prevention & Detection

Equipped with flood detection system, it will quickly detect water leaks, excess water and automatically activate the security features that the user has programmed to minimize damages and even notify you of any anomaly.

### LED Indicator

Its design features a LED that indicates if the module is currently powered on and the connection state with GroNode (the system's core module).

### Module Communication

SoilBot communicates with GroNode (the system's core module) through radio frequency with a range of 25 meters indoors (depending on obstacles) and 100 meters in open spaces. This makes it easy to install the TankBot close to the water tank.

SoilBot Specifications
Dimensions

91mm x 91mm x 28.7mm

Exterior

Casing: Stainless Steel

Colors: Silver

Physical buttons: Reset

Power Supply

USB - 5VDC 1000mA

Connections

USB 2.1 type B

RP-SMA female

Power Entry 12V/1A 24V/2A

4 x Moisture Sensor (2.5mm 4-Pin male)

2 x Temperature Sensor (2.5mm 4-Pin male)

2 x Flood Detector (2.5mm 4-Pin male)

Antenna Included

Yes

USB Cable Included

Yes (Type B-A)

USB Cable Length

2 meters

USB Power Supply Adapter Included

Yes

Sensors Included

2 x Moisture Sensor

Temperature Sensor

Flood Detector

Inter-Module Communication

Radio Frequency - 2.4GHz

Visual Indicators

LED

Warranty

2-years limited hardware warranty

SoilBot Instruction Manual

Moisture Sensor Specifications
Dimensions

13mm x 99.89mm x 2.5mm

Exterior

Material: FR-4

Colors: Pigment Green

Cable Length

2 meters

Moisture Range

5% ~ 100%

Moisture Precision

Variable (calibration dependent)

Compatibility

GroLab SoilBot

Warranty

1-year limited hardware warranty

Temperature Sensor Specifications
Dimensions
50mm (length) x 10mm (diameter)
Exterior

Casing: Stainless Steel

Colors: Silver

Cable Length
2 meters
Waterproof
Yes
Temperature Range
-40ºC ~ 110ºC
Temperature Precision
±0.5ºC
Warranty
1-year limited hardware warranty