### THE COMPLETE ALL IN ONE POWER MODULE

PowerBot allows you to connect and control the electrical peripherals of your growing environment. This powerful unit monitors and automates all the basic elements of your grow like temperature, humidity, air flow, lighting and irrigation. Create safety protocols & procedures to avoid overheating and minimize the damage in case of fire. With PowerBot every variable is under your direct control, enabling you to maximize your growth and efficiency!

### Power Supplier

PowerBot provides power to all peripherals of your growing environment. It has 4 universal outlets that supports up to 2300W (per outlet and in total) or unlimited power when using an external electrical contactor.

### Lighting

Automate any lighting system connected to PowerBot. With our advanced lightning system you are not bound to the 24 hours combined day, your grow(s) can now have a 20 hours of combined day/night, or even less if you wish so.

### Climate

The included temperature & humidity sensor and the capacity to independently control the electrical devices, allows you to perform a precise climate automation in your grow(s).

### Irrigation

From drip systems to hydroponics, GroLab™ schedule capabilities allow you to pre set the irrigation for any kind of system.

### Manual Control

This module comes with 4 external switches that give the user the ability to manually control all connected peripherals at any time on the spot.

### LED Indicator

Its design features 4 LEDs that indicates which elements are ON. Useful to visually understand what is happening on your grow(s).

### Safety Protocols & Procedures

PowerBot allows you to create safety protocols & procedures to avoid risk situations or even react to them in order to minimize the damage. The cool-down feature prevents damage to devices that need some time to cool down before turning them on (HPS Lamps).

### Wireless

PowerBot communicates with GroNode through radio frequency with a range of 25 meters indoors (depending on obstacles) and 100 meters in open spaces. This makes it easy to install the PowerBot on your growing area or even on the outside.

PowerBot Specifications
Dimensions

236.4mm x 91.4mm x 46.7mm

Exterior

Casing: Stainless Steel

Colors: Silver

Physical buttons: On/Off Switch, Reset, 4 x Outlet Controller

Power Supply

EU - 230v AC

US - 120v AC

Fuse Included

Yes (250V 16A)

Cord Included

Yes (Universal)

Cord Length

2 meters

Connections

USB 2.1 type B

RP-SMA female

Power Entry IEC 320-C14

2.5mm 4-Pin male

Antenna Included

Yes

USB Cable Included

Yes (Type B-A)

USB Cable Length

2 meters

Outlets

4 x Universal

Outlet Maximum Power

EU - 2300W(10A)

US - 1200W(10A)

Total Maximum Power

EU - 2300W(10A)

US - 1200W(10A)

Temperature & Humidity Sensor Included

Yes

Inter-Module Communication

Radio Frequency - 2.4GHz

Visual Indicators

4 x LED

Warranty

2-years limited hardware warranty

PowerBot Instruction Manual

Temperature & Humidity Sensor Specifications
Dimensions

27mm x 58.75mm x 13.30mm

Exterior

Casing: Plastic

Colors: White

Cable Length

2 meters

Temperature Range

-40ºC ~ 80ºC

Temperature Precision

±0.5ºC

Humidity Range

0% ~ 99.9%

Humidity Precision

±2%

Compatibility

GroLab PowerBot

Warranty

1-year limited hardware warranty