PH Online Probe Specifications
Dimensions

182.2mm (length) x 25.6mm (diameter)

Exterior

Casing: Plastic

Colors: Black

Cable Length

1.5 meters

Measure Range

0PH ~ 14PH

Measuring Temperature

0ºC ~ 80ºC

Resolution

0.01PH

Accuracy

±0.01PH

Drift degree

≤0.02pH/24hours

Isoelectric Point of Electrode

7±0.5PH

Response Time

<5s

Mounting Type

NPT 3/4 ″thread

Connector

BNC

Compatibility

GroLab TankBot

Warranty

1-year limited hardware warranty