# What devices and sensors can I connect to PowerBot?

In it's core, PowerBot can sample Air Temperature and Air Humidity, and comes with a probe for this purpose. It also has a internal temperature sensor for security purposes.

AIR TEMP/HUMI PROBE

Besides that, PowerBot comes with 4 controlled outputs that can turn on or off most of your grow devices.

### Outputs

Each PowerBot output can turn on/off any device that operates at 230VAC/110VAC, and does not consume more then 10A. Here are some examples of devices you can connect to your PowerBot...

BALLASTS & LAMPS

EXTRACTORS

WATER PUMPS

VAPORIZERS

CO2 DISPENSERS

...

# What devices and sensors can I connect to TankBot?

In it's core, TankBot can sample EC/pH and Water Temperature, these are static inputs available in any TankBot, this kit comes by default with a pH Probe and Water Temperature Probe.

WATER TEMPERATURE PROBE

PH PROBE

EC PROBE

Besides that, TankBot comes with 4 controlled outputs and 4 switched inputs. All of them fully configurable via the GroLab™ Software.

### Outputs

Each TankBot output can turn on/off any device that works at 12VDC that does not consume more then 6W. Here are some examples of devices you can connect to your TankBot...

PERISTALTIC PUMPS

ANY KIND OF SOLENOID

DC WATER PUMPS

POWER RELAY

...

### Inputs

Each TankBot can sense up to 4 switched inputs, what to connect to this inputs is up to you, from water level detectors, smoke detectors or even simple buttons, GroLab™ allows you to sample these sensors and act accordingly. Below you can see some of the switch sensors you can use...

LEVEL SENSORS

SMOKE DETECTORS

MOTION DETECTORS

BUTTONS

# What sensors can I connect to SoilBot?

SoilBot is a sample only purpose module, in it's core, it can sample 2 Soil/Air/Water Temperature, up to 4 Moisture sensors and also 2 Flood detectors.

The SoilBot Kit comes by default with 2 Moisture Sensors, 1 Temperature Sensor and 1 Flood Detector.

SOIL/AIR/WATER TEMPERATURE PROBE

MOISTURE PROBE

FLOOD DETECTOR

All these sensors are supplied with a 4 pin quick connector that connects directly to SoilBot, make it possible to assemble the SoilBot Kit in a matter of minutes.